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This manual describes how to use this camera. Be sure that you have read and understood its contents before using the camera.
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 Product Description:
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Waterproof Rating : IP64 ( IP64: Fully dust tight and complete protection against solid objects; Protection assured against water splashing from any angle.)
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	No using underwater
	No using in torrential rain weather
	 Allow using in light rain weather


Mounts Description :
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1/4” screw mount : Add a 1/4” screw mount could work on Bike/Motorcycle/Car ( Excluded ) 

 Get Started:
Step 1. Please fully charge the camera before the first time of using ( takes about 4 hours).

Step 2. Inserted a formatted memory card , user only a high speed Class 10 Fat formatted Micro SD Memory Card ( ≤32GB choose Fat32 format; ≥64GB choose exFat format)

FORMATE SD CARD ON PC

→ User a card reader connect the sd card to PC 

→ You could get a New “USB DRIVE” on Computer
→ Right-click “USB DRIVE", selects "Format" to complete format.  ( ≤32GB choose Fat32 format; ≥64GB choose exFat format)


    If you do not have a card reader , you could insert the sd card to camera , and connect the camera to PC to format the sd card . 

CAMERA CHARGING
→ Plug to an external 5V1A/2A wall charger,computer or power bank with the USB cable provided.

→ RED LED light is ON while charging; 

once camera is fully charged , RED LED
light turns OFF. ( takes about 

4 hours)

Power Less

When battery is in low capacity :

A RED LED light is flashing until the battery died out then the camera shuts down. 

To avoid adverse effects, please do not use a high 
  voltage charger.

TIMESTAMP SETTING

(24-hour clock）
→ Inserted a memory card

→ Connect camera to computer 

via provided USB cable ( BLUE LED is solid on )

→ A new USB Disk appears on your PC , camera will create a “txt” file (Timestamp.txt) in the new disk .

→ Open the “txt” file (Timestamp.txt) to revise the display time / date on your video.

The format is : 

	[DATE]

YEAR=2021

MONTH=06

DAY=01

HOUR=23

MINUTE=59

SECOND=59

DATE_STAMP Display=Y
	[DATE]

YEAR=2021

MONTH=06

DAY=01

HOUR=23

MINUTE=59

SECOND=59

DATE_STAMP Display=N

	Note:

1.If you do not want to show the time stamp on videos/images, You could change Y to N.

2.MONTH/ DAY / HOUR / MINUTE / SECOND except YEAR should be typed in a two-digit format,such as 01,02,03, instead of 1,2,3.

3.Please judge video " timestamp " whether the time set has been changed successfully from the new recorded.Cause the TXT files' time will not change after upgrading the camera.


→ Save the file after revising.

→ Remove the camera from computer , then Turn on the camera to upgrade the time-stamp.

	Q1
	I could not get a new disk on PC. And the GREEN LED is soid on . 

	A1
	Detect sd card , You need take off the sd card from camera, then use a card reader to format ( ≤32GB choose Fat32 format; ≥64GB choose exFat format) the sd card on computer. After that inserted the formatted sd card into the camera and reboot it . 


Audio Recording

→ Inserted a memory card

→ Long press the   button to power on and start audio recording ( A GREEN LED light is flashing during recording )
→ Press once    button to stop recording ( the flashing GREEN LED light turn to sold on ), press again to record a new audio file.

**Click one time   button could switch to video recording**
→ Long Press once    button to power off the camera



Video Recording

→ Inserted a memory card

→ Long press the   button to power on and start video recording ( A BLUE LED light is flashing during recording )
→ Press once    button to stop recording ( the flashing BLUE LED light turn to sold on ), press again to record a new video file.

**Click one time   button could switch to audio recording**
→ Long Press once    button to power off the camera




   For long time recording ,the video streaming is saved and divided into separate clips each 5 Minutes and continues recording until stopped.
Turn OFF/ON Working LED 

→ Press    and    button at the same time to power on/off  the Working LED 
Playback Videos & Audios on PC :
Media player software on Computer : VLC Media Player
Downloaded link : https://www.videolan.org/vlc/
→ Connect camera to computer 

via provided USB cable ( BLUE LED  is 

solid on )

Or : Take off the SD card from

 camera , and use a card reader 

connect it to PC )
→ A new USB Disk appears on your PC 

→ Open the “DCIM” file to view the videos & audios

  The camera do not support recording while the camera connect with computer.

	Q1
	Could i playback the videos on smartphone ? 

	A1
	Yep , but you need have card reader ( excluded )  which supports SD/Micro SD/SDHC/SDXC/MMC, Compatible for smartphone system ( such as : MacBook Pro, MacBook Air, iPad Pro 2018, Galaxy S20, Huawei Mate 30, and More ) .


 RELEVANT PARAMETERS:
	Features

	Multi-Purpose Camera , for body wearable ; cycling ; dash camera 
Audio recording mode and video recording mode 
FHD 1080P 30 FPS resolution
130 wide view angle 
Auto night vision ON/OFF
Rechargeable battery , battery life about 5 hours 
Max support 128GB micro sd card 
7/24 hours long time recording when connect with power source

	Item
	Specifications

	Video resolution 
	1920x1080P @ 30 Fps ; MP4

	Video format
	H.264

	Audio format
	WAV

	Mic rec distance
	~3 meters

	Len viewing angle
	130 degree

	IR Infrared light  
	8 PCS

	Night vision distance
	~4 meters

	Waterproof Rating
	IP64

	Power supply 
	DC 5V 1A/2A ; Battery 

	Battery capacity
	1050mah

	Battery life 
	~5 hours ( IR OFF ) ; ~ 3 hours ( IR ON )

	Storage
	Micro SD Card ( excluded ) , max support 128GB 

	
	1GB could record about 15 minutes

	Interface
	Type-C port , clip , 1/4” screw

	Camera Size
	7cmx4.5cmx2cm

	Camera Weight
	60g


Multi-Purpose Camera
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